- 3.3V Regulator installed and tested on breadboard, ADCs seem much better at this voltage, will implement on next revision.
- Pi can possibly run faster if told to explicitly, but shouldn't need to as current speed is (I think) sufficient for 10-12 datapoints in the width of one bubble
- Will attempt 3.3V ADCs on prototype board
- Working on replacing ADCs on prototype boards that are suspected to be dead
- Moving future purchases to new worktag